|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Machining stage difference | A | B | D | E |
| Dial slant height(mm) | 1.8 | 1.75 | 2.3 | 2.3 |
| Centre body thickness(mm) | 6.7 | 6.7 | 7.2 | 7.2 |
| Lug bottom to BC butting(mm) | 1.4 | 1.4 | 0.9 | 0.9 |
| Dial slant | Diamond cut | Fine turned | Diamond cut | Diamond cut |
| Dial slant angle | 24 Degree | 29 Degree | 19 Degree | 19 Degree |
| CRM length(mm) | 3.87 | B=3.88 |  | 4.3 |

**Difference between different variants**